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Uplink frequency  GHz 14.25

Downlink frequency  GHz 11.95

Carrier bandwidth kHz 26999

Uplink:

Nominal E/S e.i.r.p. per carrier  dBW 81.6

Earth station diameter  m 6.1

Earth station gain   dBi 57.3

Uplink input power per carrier   dBW 24.3

Uplink input power density dBW/Hz -50.1

Atmospheric loss   dB 0.2

Free space path loss  dB 207.2

G/T satellite  (-3 dB contour) dB/K 2.6

C/N thermal uplink  dB 31.1

C/I XPOL, ACI, ASI dB 27.0

C/(N+I) uplink   dB 25.5

Downlink:

Satellite e.i.r.p. per carrier (-3 dB contour) dBW 53.3

Atmospheric loss   dB 0.1

Free space path loss  dB 205.7

Earth station pointing loss  dB 0.3

Earth station diameter  m 0.75

Earth station gain   dBi 37.6

Noise temperature  K 120.0

Earth station G/T   dB/K 16.8

C/N thermal downlink  dB 18.3

C/I XPOL, ACI, IM, ASI dB 26.3

C/(N+I) downlink  dB 17.1

Overall:

C/(N+I) overall   dB 16.5

C/(N+I) required  dB 5.7

Margin   dB 10.8


