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Uplink frequency  GHz 14.25

Downlink frequency  GHz 11.95

Carrier bandwidth kHz 54.7

Uplink:

Nominal E/S e.i.r.p. per carrier  dBW 40.2

Earth station diameter  m 1.2

Earth station gain   dBi 43.2

Uplink input power per carrier   dBW -3.0

Uplink input power density dBW/Hz -50.4

Atmospheric loss   dB 0.2

Free space path loss  dB 207.2

G/T satellite  (-3 dB contour) dB/K 2.6

C/N thermal uplink  dB 16.6

C/I XPOL, ACI, ASI dB 26.7

C/(N+I) uplink   dB 16.2

Downlink:

Satellite e.i.r.p. per carrier (-3 dB contour) dBW 23.0

Atmospheric loss   dB 0.1

Free space path loss  dB 205.7

Earth station pointing loss  dB 0.3

Earth station diameter  m 1.2

Earth station gain   dBi 41.7

Noise temperature  K 120.0

Earth station G/T   dB/K 20.9

C/N thermal downlink  dB 19.0

C/I XPOL, ACI, IM, ASI dB 14.7

C/(N+I) downlink  dB 13.3

Overall:

C/(N+I) overall   dB 11.5

C/(N+I) required  dB 5.7

Margin   dB 5.8


