Attachment A 

The proposed antennas have the following gain pattern due to improved sidelobes as compared to the earth station antenna performance standards under 25.209
	Off-axis gain
	unit
	Off-axis angel

	29-25log(θ)
	dBi
	for       2°≤θ≤7°

	8 
	dBi
	for      7°<θ≤9.2°

	32-25log(θ)
	dBi
	for   9.2°<θ≤19.1°

	-15 
	dBi
	for    19.1°<θ≤45°

	-20 
	dBi
	for    45°<θ≤180°


