PACIFIC DATAPORT INC.

Eagle Mountain Utah – Earth Station 

Earth Station operating bands Section 24-Main Form, FCC Form 312
Transmit -28000-29100MHZ
Transmit -29300-30000MHZ
Receive -18200-19400MHZ
Receive -19600-20200MHZ
